B E I P R S T V W

## S

sDevice - Static variable in class tw.com.prolific.driver.pl2303g.PL2303GDriver
setDTR(boolean) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Switch PL2303G DTR on or off
setRTS(boolean) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Switch PL2303G RTS on or off
setup(PL2303GDriver.BaudRate, PL2303GDriver.DataBits, PL2303GDriver.StopBits, PL2303GDriver.Parity, PL2303GDriver.FlowControl) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Setup basic communication parameters on PL2303G chip

B E I P R S T V W