## Uses of Class
tw.com.prolific.driver.pl2303g.PL2303GDriver.Parity

- - ### Uses of PL2303GDriver.Parity in tw.com.prolific.driver.pl2303g

    Methods in tw.com.prolific.driver.pl2303g that return PL2303GDriver.Parity
    Modifier and Type | Method and Description
    --- | ---
    `static PL2303GDriver.Parity` | PL2303GDriver.Parity.`valueOf(java.lang.String name)` Returns the enum constant of this type with the specified name.
    `static PL2303GDriver.Parity[]` | PL2303GDriver.Parity.`values()` Returns an array containing the constants of this enum type, in the order they are declared.

    Methods in tw.com.prolific.driver.pl2303g with parameters of type PL2303GDriver.Parity
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | PL2303GDriver.`InitByPortSetting(PL2303GDriver.BaudRate R, PL2303GDriver.DataBits D, PL2303GDriver.StopBits S, PL2303GDriver.Parity P, PL2303GDriver.FlowControl F)` Open an PL2303G USB Device by BaudRate, Data bit, stop bit, parity bit and Flow Control
    `int` | PL2303GDriver.`setup(PL2303GDriver.BaudRate R, PL2303GDriver.DataBits D, PL2303GDriver.StopBits S, PL2303GDriver.Parity P, PL2303GDriver.FlowControl F)` Setup basic communication parameters on PL2303G chip